# Data Movement These instructions move data from one place to another.
EXG | The contents of two registers will be exchanged.
LEA | Calculates a memory location and stores it into an address register.
LINK | Allocates a stack frame.
MOVE | Copies the contents in one register/memory location into another register/memory location.
MOVEA | Same as MOVE except that the destination is an address-register.
MOVEM | transfers many registers to or from the memory.
MOVEP | transfers data to or from an 8 bit peripheral unit.
MOVEQ | puts a constant in a data register.
PEA | calculates a memory address and stores it on the stack.
SWAP | Swaps the low and high words in a data register.
UNLK | removes a stack frame
###  |