Sim68K - Memory Window

The simulator provides a full 16 Mega Byte 68000 address space from address $00000000 - $00FFFFFF. To view the 68000's memory select Memory from the View menu.

Each row of the memory window displays an address followed by 16 bytes of hexadecimal memory data, followed by the ASCII representation of the 16 bytes. The contents of memory may be changed by clicking on the desired location and entering a new value. Entries may be made in Hexadecimal or ASCII. Use the Row and Page buttons or the mouse wheel to scroll up or down through memory. To jump to a certain address, enter it in the Address: field.

Copy
Blocks of memory may be copied. Enter the From and To address and the number of Bytes to copy and click the Copy button. Memory copy is useful when testing position independent code.

Fill
Blocks of memory may be filled. Enter the From and To address and the Bytes to fill with and click the Fill button.

Blocks of memory may be saved to a binary file. Enter the From and To address and click the Save button.

Live
When checked the memory window presents a live view of 68000 memory.

* All numbers are entered in hexadecimal.