Sim68K - Stack Window

The 68000's stack space may be viewed by selecting Stack from the View menu.

Address registers A0 - A6, User Stack (US) or System Stack (SS) may be selected as the stack pointer. The stack space is displayed for the currently selected register. The location of the selected register is highlighted in blue and the location of the current system stack is highlighted in yellow. Use the Up/Down buttons or scroll wheel on the mouse to move through stack memory. Memory ranges in the Invalid address space as specified on the Hardware window are displayed in red.